Notes taken from Lab 1 Activity 28:00-32:00

1. Stairs cannot go smaller when they go down
2. Increase like corridor and radge
3. Egress of stairways
   1. 0.3 in per occupant
   2. 0.2 in per occupant in building with sprinklered system and an emergency alarm communication system
   3. Compared with the listed minimum width in code(IBC 44’ for more than 50 people)
   4. Distribution of egress capacity should be listed, either of the egress should be at least above half of the capacity
4. Egress of corridor
   1. 0.2 in per occupant
   2. 0.15 in per occupant for sprinklered section
   3. Minimum of 44’
5. Egress of Door
   1. 0.2 in per occupant
   2. 0.15 in per occupant for sprinklered section
   3. Minimum of 32’
6. Requirements for the remoted exit
   1. For buildings need more than one exit
   2. Requirements on the travel distance